| Demo HCI Implementation for WiMOD-LR Devices V1.3.1

- Main Page
- Classes
- Files

- File List
- File Members

Classes | Typedefs
WiMODLR_BASE.h File Reference

Declarations for the High-level Interface for WiMOD LR-Base firmware. More...

`#include "Arduino.h"`
`#include <string.h>`
`#include "utils/WMDefs.h"`
`#include "utils/ComSLIP.h"`
`#include "HCI/WiMODLRHCI.h"`
`#include "SAP/WiMOD_SAP_DEVMGMT.h"`
`#include "SAP/WiMOD_SAP_RadioLink.h"`
`#include "SAP/WiMOD_SAP_HWTest.h"`
`#include "utils/FreqCalc.h"`
Include dependency graph for WiMODLR_BASE.h:
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Classes
class | WiMODLRBASE
| Main class representing the interface to the WiMOD running the firmware WiMODLR-BASE. More...

## Typedefs
typedef void(* | TDataLinkRxUDataIndClient) (UINT8 *data, UINT16 length)
typedef void(* | TDataLinkSendUdataIndClient) (UINT8 status)

## Detailed Description

Declarations for the High-level Interface for WiMOD LR-Base firmware.

Version
  0.1

Author
  (FB), IMST

## Typedef Documentation

typedef void(* TDataLinkRxUDataIndClient) (UINT8 *data, UINT16 length)

THIS IS AN EXAMPLE IMPLEMENTATION ACCORDING THE THE HCI SPEC: V1.8 FOR FIRMWARE: LR-BASEType definition for callback function that handles a 'RX U-Data event' for the DataLink service

typedef void(* TDataLinkSendUdataIndClient) (UINT8 status)

Type definition for callback function that handles a 'TX U-Data event' for the DataLink service