| Demo HCI Implementation for WiMOD-LR Devices V1.3.1

- Main Page
- Classes
- Files

- Class List
- Class Hierarchy
- Class Members

Public Attributes | List of all members
TWiMODLORAWAN_RadioStackConfig Struct Reference

Radio stack configuration related to to LoRaWAN specific options. More...

`#include <SAP/WiMOD_SAP_LORAWAN_IDs.h>`

## Public Attributes
UINT8 | DataRateIndex
UINT8 | TXPowerLevel
UINT8 | Options
UINT8 | PowerSavingMode
UINT8 | Retransmissions
UINT8 | BandIndex

## Detailed Description

Radio stack configuration related to to LoRaWAN specific options.

## Member Data Documentation

UINT8 TWiMODLORAWAN_RadioStackConfig::BandIndex

Frequency band to use (

See also
  TLoRaWAN_FreqBand)

UINT8 TWiMODLORAWAN_RadioStackConfig::DataRateIndex

data rate to use (

See also
  TLoRaWANDataRate)

UINT8 TWiMODLORAWAN_RadioStackConfig::Options

misc Options (see LORAWAN_STK_OPTION defines)

UINT8 TWiMODLORAWAN_RadioStackConfig::PowerSavingMode

set automatic power saving mode

UINT8 TWiMODLORAWAN_RadioStackConfig::Retransmissions

max number of retransmissions (for C-Data) to use

UINT8 TWiMODLORAWAN_RadioStackConfig::TXPowerLevel

default / initial power level settings to be used

The documentation for this struct was generated from the following file:

- SAP/WiMOD_SAP_LORAWAN_IDs.h