| Demo HCI Implementation for WiMOD-LR Devices V1.3.1

- Main Page
- Classes
- Files

- Class List
- Class Hierarchy
- Class Members

WiMODLRBASE Member List

This is the complete list of members for WiMODLRBASE, including all inherited members.

begin(void) | WiMODLRBASE | virtual
calcFreqToRegister(uint32_t freq, uint8_t *msb, uint8_t *mid, uint8_t *lsb) | WiMODLRBASE |
calcRegisterToFreq(uint8_t msb, uint8_t mid, uint8_t lsb) | WiMODLRBASE |
ClearRtcAlarm(TWiMDLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE |
convert(TWiMODLR_HCIMessage &RxMsg, TWiMODLR_RadioLink_Msg *radioLinkMsg) | WiMODLRBASE |
convert(TWiMODLR_HCIMessage &RxMsg, TWiMODLR_RadioLink_CdataInd *cDataTxInfo) | WiMODLRBASE |
convert(TWiMODLR_HCIMessage &RxMsg, TWiMODLR_AckTxInd_Msg *txAckIndInfo) | WiMODLRBASE |
copyResultInfos(TWiMDLRResultCodes *hciResult, UINT8 *rspStatus, UINT8 successValue) | WiMODLRBASE | protected
end(void) | WiMODLRBASE | virtual
GetAesKey(UINT8 *key, TWiMDLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE |
GetDeviceInfo(TWiMODLR_DevMgmt_DevInfo *info, TWiMDLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE |
GetFirmwareInfo(TWiMODLR_DevMgmt_FwInfo *info, TWiMDLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE |
GetLastHciResult(void) | WiMODLRBASE |
GetLastResponseStatus(void) | WiMODLRBASE |
GetOperationMode(TWiMOD_OperationMode *opMode, TWiMDLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE |
GetRadioConfig(TWiMODLR_DevMgmt_RadioConfig *radioCfg, TWiMDLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE |
GetRtc(UINT32 *rtcTime, TWiMDLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE |
GetRtcAlarm(TWiMODLR_DevMgmt_RtcAlarm *rtcAlarm, TWiMDLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE |
GetRxMessage(void) | TWiMODLRHCI |
GetSystemStatus(TWiMODLR_DevMgmt_SystemStatus *info, TWiMDLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE |
Ping(TWiMDLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE |
Process(void) | TWiMODLRHCI |
ProcessRxMessage(UINT8 *, UINT16) (defined in TComSlipClient) | TComSlipClient | inline virtual
ProcessUnexpectedRxMessage(TWiMODLR_HCIMessage &rxMsg) | WiMODLRBASE | protected virtual
RegisterAckRxClient(TRadioLinkAckRxIndicationCallback cb) | WiMODLRBASE |
RegisterAckRxTimeoutClient(TRadioLinkAckRxTimeoutIndicationCallback cb) | WiMODLRBASE |
RegisterAckTxCallback(TRadioLinkAckTxIndicationCallback cb) | WiMODLRBASE |
RegisterCDataRxClient(TRadioLinkCDataRxIndicationCallback cb) | WiMODLRBASE |
RegisterCDataTxClient(TRadioLinkCDataTxIndicationCallback cb) | WiMODLRBASE |
RegisterPowerUpIndicationClient(TDevMgmtPowerUpCallback cb) | WiMODLRBASE |
RegisterRawDataRxClient(TRadioLinkRawDataRxIndicationCallback cb) (defined in WiMODLRBASE) | WiMODLRBASE |
RegisterRtcAlarmIndicationClient(TDevMgmtRtcAlarmCallback cb) | WiMODLRBASE |
RegisterStackErrorClient(TWiMODStackErrorClient cb) | TWiMODLRHCI |
RegisterUDataRxClient(TRadioLinkUDataRxIndicationCallback cb) | WiMODLRBASE |
RegisterUDataTxClient(TRadioLinkUDataTxIndicationCallback cb) | WiMODLRBASE |
Reset(TWiMDLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE |
ResetRadioConfig(TWiMDLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE |
SapDevMgmt | WiMODLRBASE | protected
SapRadioLink | WiMODLRBASE | protected
SendCData(const TWiMODLR_RadioLink_Msg *txMsg, TWiMDLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE |
SendHCIMessage(UINT8 dstSapID, UINT8 msgID, UINT8 rxMsgID, UINT8 *payload, UINT16 length) | TWiMODLRHCI |
SendUData(const TWiMODLR_RadioLink_Msg *txMsg, TWiMDLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE |
SendWakeUpSequence(void) | TWiMODLRHCI |
SetAckData(const TWiMODLR_RadioLink_Msg *txMsg, TWiMDLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE |
SetAesKey(const UINT8 *key, TWiMDLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE |
SetOperationMode(const TWiMOD_OperationMode opMode, TWiMDLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE |
SetRadioConfig(const TWiMODLR_DevMgmt_RadioConfig *radioCfg, TWiMDLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE |
SetRtc(const UINT32 rtcTime, TWiMDLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE |
SetRtcAlarm(const TWiMODLR_DevMgmt_RtcAlarm *rtcAlarm, TWiMDLRResultCodes *hciResult=NULL, UINT8 *rspStatus=NULL) | WiMODLRBASE |
TComSlipClient() (defined in TComSlipClient) | TComSlipClient | inline
TWiMODLRHCI(Stream &s) | TWiMODLRHCI |
WiMODLRBASE(Stream &s) | WiMODLRBASE |
~TComSlipClient() (defined in TComSlipClient) | TComSlipClient | inline virtual
~TWiMODLRHCI(void) | TWiMODLRHCI |
~WiMODLRBASE(void) | WiMODLRBASE |