| Demo HCI Implementation for WiMOD-LR Devices V1.3.1

- Main Page
- Classes
- Files

- Class List
- Class Hierarchy
- Class Members

Class List
Here are the classes, structs, unions and interfaces with brief descriptions:

C CayenneLPP |
C TComSlip | Class for handling SLIP encoding and decoding of HCI messages
C TComSlipClient | Class definition for enabling OO inheritance
C TWiMODLORAWAN_ActivateDeviceData | Activation data structure for LoRa network activation
C TWiMODLORAWAN_JoinParams | JOIN data structure for LoRa network activation
C TWiMODLORAWAN_MacCmd | LoRaWAN MAC command structure
C TWiMODLORAWAN_NwkStatus_Data | Structure containing all data about LoRaWAN network status
C TWiMODLORAWAN_RadioStackConfig | Radio stack configuration related to to LoRaWAN specific options
C TWiMODLORAWAN_RX_ACK_Data | Data structure for received Acknowledgment data
C TWiMODLORAWAN_RX_Data | Structure containing RX (user) payload data
C TWiMODLORAWAN_RX_JoinedNwkData | Structure containing data of the joined network indication
C TWiMODLORAWAN_RX_MacCmdData | Structure containing a received MAC command
C TWiMODLORAWAN_TX_Data | Structure containing all data necessary to transmitting a data message
C TWiMODLORAWAN_TxIndData | Activation data structure for LoRa network activation
C TWiMODLR_AckTxInd_Msg | Structure containing information about an acknowledgment transmission
C TWiMODLR_DevMgmt_DevInfo | Structure containing basic information about the WiMOD device
C TWiMODLR_DevMgmt_FwInfo | Basic information about the current firmware of the WiMOD
C TWiMODLR_DevMgmt_RadioConfig | Structure containing the radio (stack) config parameters of the WiMOD (only for LR-BASE)
C TWiMODLR_DevMgmt_RtcAlarm | Structure containing the RTC Alarm config parameters of the WiMOD
C TWiMODLR_DevMgmt_SystemStatus | Basic information about system status of the WiMOD
C TWiMODLR_HCIMessage | Basic low level HCI message structure used for all serial messages to/from WiMOD
C TWiMODLR_RadioLink_CdataInd | Structure containing information about a C-Data indication (TX only)
C TWiMODLR_RadioLink_Msg | Structure containing a general RadioLink HCI message
C TWiMODLRHCI | Internal helper class for processing SLIP frames
C TWiMODLRHCIClient | Internal helper class for processing HCI frames
C WiMOD_SAP_DevMgmt | Implementation for the ServiceAccessPoint DeviceManagement
C WiMOD_SAP_LoRaWAN | Implementation for the ServiceAccessPoint LoRaWAN (End Node Modem firmware only)
C WiMOD_SAP_RadioLink | Implementation for the ServiceAccessPoint RadioLink (LR-Base firmware only)
C WiMODLoRaWAN | Main class representing the interface to the WiMOD running the firmware LoRaWAN EndNode Modem
C WiMODLRBASE | Main class representing the interface to the WiMOD running the firmware WiMODLR-BASE