| Demo HCI Implementation for WiMOD-LR Devices V1.3.1

- Main Page
- Classes
- Files

- Class List
- Class Hierarchy
- Class Members

Public Attributes | List of all members
TWiMODLR_RadioLink_Msg Struct Reference

Structure containing a general RadioLink HCI message. More...

`#include <SAP/WiMOD_SAP_RadioLink_IDs.h>`

## Public Attributes
UINT8 | StatusFormat
UINT8 | DestinationGroupAddress
UINT16 | DestinationDeviceAddress
UINT8 | SourceGroupAddress
UINT16 | SourceDeviceAddress
UINT8 | Length
UINT8 | Payload [WIMOD_RADIOLINK_PAYLOAD_LEN]
bool | OptionalInfoAvaiable
INT16 | RSSI
INT8 | SNR
INT32 | RxTime

## Detailed Description

Structure containing a general RadioLink HCI message.

## Member Data Documentation

UINT16 TWiMODLR_RadioLink_Msg::DestinationDeviceAddress

Address of destination device this message is targeting to

UINT8 TWiMODLR_RadioLink_Msg::DestinationGroupAddress

Address of destination group this message is targeting to

UINT8 TWiMODLR_RadioLink_Msg::Length

length of the (user) payload data field

bool TWiMODLR_RadioLink_Msg::OptionalInfoAvaiable

Flag indicating if optional receiver infomation is available

UINT8 TWiMODLR_RadioLink_Msg::Payload[WIMOD_RADIOLINK_PAYLOAD_LEN]

(user) payload field

INT16 TWiMODLR_RadioLink_Msg::RSSI

RSSI value (WiMOD –> host only)

INT32 TWiMODLR_RadioLink_Msg::RxTime

RX timestamp of this message (WiMOD –> host only)

INT8 TWiMODLR_RadioLink_Msg::SNR

SNR value (WiMOD –> host only)

UINT16 TWiMODLR_RadioLink_Msg::SourceDeviceAddress

Address of source device this message was send from

UINT8 TWiMODLR_RadioLink_Msg::SourceGroupAddress

Address of source group this message was send from

UINT8 TWiMODLR_RadioLink_Msg::StatusFormat

Status/Format Field set by WiMOD; (WiMOD –> Host only)

The documentation for this struct was generated from the following file:

- SAP/WiMOD_SAP_RadioLink_IDs.h