| Demo HCI Implementation for WiMOD-LR Devices V1.3.1

- Main Page
- Classes
- Files

- Class List
- Class Hierarchy
- Class Members

CayenneLPP Member List

This is the complete list of members for CayenneLPP, including all inherited members.

addAccelerometer(uint8_t channel, float x, float y, float z) (defined in CayenneLPP) | CayenneLPP |
addAnalogInput(uint8_t channel, float value) (defined in CayenneLPP) | CayenneLPP |
addAnalogOutput(uint8_t channel, float value) (defined in CayenneLPP) | CayenneLPP |
addBarometricPressure(uint8_t channel, float hpa) (defined in CayenneLPP) | CayenneLPP |
addCustomValue(uint8_t channel, uint8_t type, uint8_t valueSize, uint8_t *value) (defined in CayenneLPP) | CayenneLPP |
addDigitalInput(uint8_t channel, uint8_t value) (defined in CayenneLPP) | CayenneLPP |
addDigitalOutput(uint8_t channel, uint8_t value) (defined in CayenneLPP) | CayenneLPP |
addGPS(uint8_t channel, float latitude, float longitude, float meters) (defined in CayenneLPP) | CayenneLPP |
addGyrometer(uint8_t channel, float x, float y, float z) (defined in CayenneLPP) | CayenneLPP |
addLuminosity(uint8_t channel, uint16_t lux) (defined in CayenneLPP) | CayenneLPP |
addPresence(uint8_t channel, uint8_t value) (defined in CayenneLPP) | CayenneLPP |
addRelativeHumidity(uint8_t channel, float rh) (defined in CayenneLPP) | CayenneLPP |
addTemperature(uint8_t channel, float celsius) (defined in CayenneLPP) | CayenneLPP |
CayenneLPP(uint8_t *buf, uint8_t size) (defined in CayenneLPP) | CayenneLPP |
copy(uint8_t *buffer) (defined in CayenneLPP) | CayenneLPP |
getBuffer(void) (defined in CayenneLPP) | CayenneLPP |
getSize(void) (defined in CayenneLPP) | CayenneLPP |
reset(void) (defined in CayenneLPP) | CayenneLPP |
~CayenneLPP() (defined in CayenneLPP) | CayenneLPP |