| Demo HCI Implementation for WiMOD-LR Devices V1.3.1

- Main Page
- Classes
- Files

- File List
- File Members

WiMOD_SAP_HWTest.h
1 //------------------------------------------------------------------------------
31 //------------------------------------------------------------------------------
32
33
34 /*
35 * THIS IS AN EXAMPLE IMPLEMENTATION ACCORDING THE THE HCI SPEC: V1.8
36 * FOR FIRMWARE: LR-BASE
37 *
38 * SEE FILE: WiMOD_LR_Base_HCI_Spec_V1_8.pdf for detailed information
39 */
40
41 #if 0 /* This should not part of the normal production code */
42
43 #ifndef ARDUINO_SAP_WIMOD_SAP_HWTEST_H_
44 #define ARDUINO_SAP_WIMOD_SAP_HWTEST_H_
45
46 #include "WiMOD_SAP_HWTest_IDs.h"
47 #include "../HCI/WiMODLRHCI.h"
48
49 /*
50 * C++11 supports a better way for function pointers / function objects
51 * But C++11 mode is not supported by all platforms.
52 */
53 #ifdef WIMOD_USE_CPP11
54 #include <functional>
55 #endif
56 //------------------------------------------------------------------------------
57 //
58 // Section defines
59 //
60 //------------------------------------------------------------------------------
62 #define WiMOD_DEVMGMT_MSG_SIZE (100)
63
64
65 //-----------------------------------------------------------------------------
66 //
67 // types for callback functions
68 //
69 //-----------------------------------------------------------------------------
70
71 // C++11 check
72 #ifdef WIMOD_USE_CPP11
73 /* C++11 function callback definitions */
74
76 typedef std::function<void (void)> TDevMgmtPowerUpCallback;
77
78 #else
79 /* pre C++11 function callback definitions */
80
82 typedef void (*TDevMgmtPowerUpCallback)(void);
83
84 #endif
85
86 //------------------------------------------------------------------------------
87 //
88 // Section class
89 //
90 //------------------------------------------------------------------------------
91
95 class WiMOD_SAP_HWTest {
96 public:
97 WiMOD_SAP_HWTest(TWiMODLRHCI* hci, UINT8* buffer, UINT16 bufferSize);
98 ~WiMOD_SAP_HWTest(void);
99
100 TWiMDLRResultCodes StartRadioTest(const TWiMODLR_HWTestParameter* testParams, UINT8* statusRsp);
101 TWiMDLRResultCodes StopRadioTest(UINT8* statusRsp);
102
103 protected:
104 private:
106 UINT8* txPayload;
107 UINT16 txyPayloadSize;
108
109 TWiMODLRHCI* HciParser;
111
112 };
113
114 #endif
115
116 #endif /* ARDUINO_SAP_WIMOD_SAP_HWTEST_H_ */
TWiMDLRResultCodes
TWiMDLRResultCodes
Result codes for the local serial communication itself.
Definition: WiMODLRHCI.h:149
TWiMODLRHCI
Internal helper class for processing SLIP frames.
Definition: WiMODLRHCI.h:229
WiMOD_SAP_HWTest_IDs.h
Supporting IDs and definitions for the hardware test ServiceAccessPoint.
TDevMgmtPowerUpCallback
void(* TDevMgmtPowerUpCallback)(void)
Definition: WiMOD_SAP_DEVMGMT.h:93