| Demo HCI Implementation for WiMOD-LR Devices V1.3.1

- Main Page
- Classes
- Files

- Class List
- Class Hierarchy
- Class Members

Public Attributes | List of all members
TWiMODLORAWAN_RX_Data Struct Reference

Structure containing RX (user) payload data. More...

`#include <SAP/WiMOD_SAP_LORAWAN_IDs.h>`

## Public Attributes
UINT8 | StatusFormat
UINT8 | Port
UINT8 | Length
UINT8 | Payload [WiMODLORAWAN_APP_PAYLOAD_LEN]
UINT8 | ChannelIndex
UINT8 | DataRateIndex
INT8 | RSSI
INT8 | SNR
UINT8 | RxSlot
bool | OptionalInfoAvaiable

## Detailed Description

Structure containing RX (user) payload data.

## Member Data Documentation

UINT8 TWiMODLORAWAN_RX_Data::ChannelIndex

used channel index (

See also
  TLoRaWAN_Channel_* definitions)

UINT8 TWiMODLORAWAN_RX_Data::DataRateIndex

used data rate index (

See also
  TLoRaWANDataRate)

UINT8 TWiMODLORAWAN_RX_Data::Length

Length of the used (user) payload field

bool TWiMODLORAWAN_RX_Data::OptionalInfoAvaiable

are the optional value fields available

UINT8 TWiMODLORAWAN_RX_Data::Payload[WiMODLORAWAN_APP_PAYLOAD_LEN]

payload data

UINT8 TWiMODLORAWAN_RX_Data::Port

(Target) LoRaWAN port

INT8 TWiMODLORAWAN_RX_Data::RSSI

RSSI value for the received packet

UINT8 TWiMODLORAWAN_RX_Data::RxSlot

number of the rx slot that contained the messsage

INT8 TWiMODLORAWAN_RX_Data::SNR

SNR value for the received packet

UINT8 TWiMODLORAWAN_RX_Data::StatusFormat

Status/Format Field for this message

The documentation for this struct was generated from the following file:

- SAP/WiMOD_SAP_LORAWAN_IDs.h