| Demo HCI Implementation for WiMOD-LR Devices V1.3.1

- Main Page
- Classes
- Files

- Class List
- Class Hierarchy
- Class Members

Public Attributes | List of all members
TWiMODLORAWAN_RX_MacCmdData Struct Reference

Structure containing a received MAC command. More...

`#include <SAP/WiMOD_SAP_LORAWAN_IDs.h>`

## Public Attributes
UINT8 | Length
UINT8 | MacCmdData [WiMODLORAWAN_APP_PAYLOAD_LEN]
UINT8 | ChannelIndex
UINT8 | DataRateIndex
INT8 | RSSI
INT8 | SNR
UINT8 | RxSlot
bool | OptionalInfoAvaiable

## Detailed Description

Structure containing a received MAC command.

## Member Data Documentation

UINT8 TWiMODLORAWAN_RX_MacCmdData::ChannelIndex

used channel index (

See also
  TLoRaWAN_Channel_* definitions)

UINT8 TWiMODLORAWAN_RX_MacCmdData::DataRateIndex

used data rate index (

See also
  TLoRaWANDataRate)

UINT8 TWiMODLORAWAN_RX_MacCmdData::Length

length of the MAC command / data

UINT8 TWiMODLORAWAN_RX_MacCmdData::MacCmdData[WiMODLORAWAN_APP_PAYLOAD_LEN]

MAC command / data

bool TWiMODLORAWAN_RX_MacCmdData::OptionalInfoAvaiable

are the optional value fields available

INT8 TWiMODLORAWAN_RX_MacCmdData::RSSI

RSSI value for the received packet

UINT8 TWiMODLORAWAN_RX_MacCmdData::RxSlot

number of the rx slot that contained the messsage

INT8 TWiMODLORAWAN_RX_MacCmdData::SNR

SNR value for the received packet

The documentation for this struct was generated from the following file:

- SAP/WiMOD_SAP_LORAWAN_IDs.h