| Demo HCI Implementation for WiMOD-LR Devices V1.3.1

- Main Page
- Classes
- Files

- Class List
- Class Hierarchy
- Class Members

Public Attributes | List of all members
TWiMODLORAWAN_NwkStatus_Data Struct Reference

Structure containing all data about LoRaWAN network status. More...

`#include <SAP/WiMOD_SAP_LORAWAN_IDs.h>`

## Public Attributes
UINT8 | NetworkStatus
UINT32 | DeviceAddress
UINT8 | DataRateIndex
UINT8 | PowerLevel
UINT8 | MaxPayloadSize

## Detailed Description

Structure containing all data about LoRaWAN network status.

## Member Data Documentation

UINT8 TWiMODLORAWAN_NwkStatus_Data::DataRateIndex

used data rate index (

See also
  TLoRaWANDataRate)

UINT32 TWiMODLORAWAN_NwkStatus_Data::DeviceAddress

32bit DeviceAddress of module in LoRa network

UINT8 TWiMODLORAWAN_NwkStatus_Data::MaxPayloadSize

maximum number of bytes allowed in payload field

UINT8 TWiMODLORAWAN_NwkStatus_Data::NetworkStatus

Current NetworkStatus (

See also
  TLoRaWAN_NwkStatus)

UINT8 TWiMODLORAWAN_NwkStatus_Data::PowerLevel

transmit power in dBm

The documentation for this struct was generated from the following file:

- SAP/WiMOD_SAP_LORAWAN_IDs.h