| Demo HCI Implementation for WiMOD-LR Devices V1.3.1

- Main Page
- Classes
- Files

- Class List
- Class Hierarchy
- Class Members

Public Attributes | List of all members
TWiMODLR_DevMgmt_RadioConfig Struct Reference

Structure containing the radio (stack) config parameters of the WiMOD (only for LR-BASE) More...

`#include <SAP/WiMOD_SAP_DEVMGMT_IDs.h>`

## Public Attributes
UINT8 | Status
UINT8 | StoreNwmFlag
TRadioCfg_RadioMode | RadioMode
UINT8 | GroupAddress
UINT8 | TxGroupAddress
UINT16 | DeviceAddress
UINT16 | TxDeviceAddress
TRadioCfg_Modulation | Modulation
UINT8 | RfFreq_LSB
UINT8 | RfFreq_MID
UINT8 | RfFreq_MSB
TRadioCfg_LoRaBandwidth | LoRaBandWidth
TRadioCfg_LoRaSpreadingFactor | LoRaSpreadingFactor
TRadioCfg_ErrorCoding | ErrorCoding
TRadioCfg_PowerLevel | PowerLevel
UINT8 | TxControl
TRadioCfg_RxControl | RxControl
UINT16 | RxWindowTime
UINT8 | LedControl
UINT8 | MiscOptions
TRadioCfg_FskDatarate | FskDatarate
TRadioCfg_PowerSavingMode | PowerSavingMode
INT16 | LbtThreshold

## Detailed Description

Structure containing the radio (stack) config parameters of the WiMOD (only for LR-BASE)

## Member Data Documentation

UINT16 TWiMODLR_DevMgmt_RadioConfig::DeviceAddress

RF device address used for RX

TRadioCfg_ErrorCoding TWiMODLR_DevMgmt_RadioConfig::ErrorCoding

Error Coding

TRadioCfg_FskDatarate TWiMODLR_DevMgmt_RadioConfig::FskDatarate

Datarate setting for the FSK modulation

UINT8 TWiMODLR_DevMgmt_RadioConfig::GroupAddress

Group address of WiMOD (for RX)

INT16 TWiMODLR_DevMgmt_RadioConfig::LbtThreshold

ListenBeforeTalk threshold value

UINT8 TWiMODLR_DevMgmt_RadioConfig::LedControl

control byte for the LED (of the demoboard)

TRadioCfg_LoRaBandwidth TWiMODLR_DevMgmt_RadioConfig::LoRaBandWidth

Bandwidth setting for the LoRa modulation

TRadioCfg_LoRaSpreadingFactor TWiMODLR_DevMgmt_RadioConfig::LoRaSpreadingFactor

LoRa Spreading factor

UINT8 TWiMODLR_DevMgmt_RadioConfig::MiscOptions

misc options field

TRadioCfg_Modulation TWiMODLR_DevMgmt_RadioConfig::Modulation

RF Modulation to be used for TX

TRadioCfg_PowerLevel TWiMODLR_DevMgmt_RadioConfig::PowerLevel

Power Level setting

TRadioCfg_PowerSavingMode TWiMODLR_DevMgmt_RadioConfig::PowerSavingMode

PowerSaving; 1 = enable/ on; 0 = disable / off

TRadioCfg_RadioMode TWiMODLR_DevMgmt_RadioConfig::RadioMode

Radio Mode setting

UINT8 TWiMODLR_DevMgmt_RadioConfig::RfFreq_LSB

lower part of the 24bit frequency register of the transceiver

UINT8 TWiMODLR_DevMgmt_RadioConfig::RfFreq_MID

mid part of the 24bit frequency register of the transceiver

UINT8 TWiMODLR_DevMgmt_RadioConfig::RfFreq_MSB

high part of the 24bit frequency register of the transceiver

TRadioCfg_RxControl TWiMODLR_DevMgmt_RadioConfig::RxControl

Options related to RX operations

UINT16 TWiMODLR_DevMgmt_RadioConfig::RxWindowTime

Time settings related to the RX Window

UINT8 TWiMODLR_DevMgmt_RadioConfig::Status

Status Flag of HCI get operation; only vaild if config has been requested

UINT8 TWiMODLR_DevMgmt_RadioConfig::StoreNwmFlag

Store the config in NVM or RAM; 1 = store in NVM

UINT8 TWiMODLR_DevMgmt_RadioConfig::TxControl

Options related to TX operations

UINT16 TWiMODLR_DevMgmt_RadioConfig::TxDeviceAddress

RF device address used for TX

UINT8 TWiMODLR_DevMgmt_RadioConfig::TxGroupAddress

Group address to be used for TX

The documentation for this struct was generated from the following file:

- SAP/WiMOD_SAP_DEVMGMT_IDs.h