| Demo HCI Implementation for WiMOD-LR Devices V1.3.1

- Main Page
- Classes
- Files

- Class List
- Class Hierarchy
- Class Members

Public Attributes | List of all members
TWiMODLORAWAN_TxIndData Struct Reference

Activation data structure for LoRa network activation. More...

`#include <SAP/WiMOD_SAP_LORAWAN_IDs.h>`

## Public Attributes
TWiMOD_OptIndInfos | FieldAvailability
UINT8 | StatusFormat
UINT8 | ChannelIndex
UINT8 | DataRateIndex
UINT8 | NumTxPackets
UINT8 | PowerLevel
UINT32 | RfMsgAirtime

## Detailed Description

Activation data structure for LoRa network activation.

## Member Data Documentation

UINT8 TWiMODLORAWAN_TxIndData::ChannelIndex

used channel index (

See also
  TLoRaWAN_Channel_* definitions)

UINT8 TWiMODLORAWAN_TxIndData::DataRateIndex

used data rate index (

See also
  TLoRaWANDataRate)

TWiMOD_OptIndInfos TWiMODLORAWAN_TxIndData::FieldAvailability

indicator flag for optional infos

UINT8 TWiMODLORAWAN_TxIndData::NumTxPackets

number of TX packet (for current operation; can be used as retransmission counter)

UINT8 TWiMODLORAWAN_TxIndData::PowerLevel

transmit power in dBm

UINT32 TWiMODLORAWAN_TxIndData::RfMsgAirtime

airtime in ms of packet transmission

UINT8 TWiMODLORAWAN_TxIndData::StatusFormat

Status/Format field of reponse packet from WiMOD

The documentation for this struct was generated from the following file:

- SAP/WiMOD_SAP_LORAWAN_IDs.h